# 2005 Emission Inventory

Log-in |

### Top Menu

Stampa: Stampa Anteprima di stampa Esporta come PDF Esporta in formato RTF Esporta come HTML Esporta in formato XAR

## 2005 Emission Inventory

- Methodology
- Typologies of atmospheric pollutant sources
- Pollutants
- Aggregated pollution indicators
- Classification of activities (SNAP 97)
- "Top-Down" and "Bottom-Up"
- Spatial disaggregation of emissions
- Temporal modulation of emissions
- Data sources
- Emission factors
- Uncertainty
- Work in progress

### Spatial disaggregation of emissions

A very common problem is the apportionment of an emission datum evaluated at an aggregated territorial level, such as a region or a nation, to a portion of territory contained in it, e.g. a county or a municipality.

This operation of disaggregation is carried out basing on some indicators, also called "surrogated variables " or "proxy variables", considered able to represent the weigh distribution of the different emission on the territory.

In order to go from a "total" value of a given emission to a "local" one, is then possible to use this formula:

El = Et * Vl / Vt (2)

where:

El = local emission;

Et = total emission;

Vl = local value of the surrogated variable;

Vt = total value of the surrogated variable.

Examples of surrogated variables are number of inhabitants, fuel consumption, industrial production, or the employees in a given sector whose emission is to be evaluated. The choice of the surrogated variable is a very sensitive element, and must also take into account the available information about emission factors.

This approach was used also in the inventory and in the INEMAR database: the disaggregation of county emissions at municipal for each activity was carried out using some proxy variables.

Example In order to explain the application of this methodology si riporta come esempio the calculation of N2O emission from the use of fertilizers on ploughed lands (activity SNAP 10.1.2) in the municipality of Dovera (CR):

ACR = indicator = use of fertilizers in the Province of Cremona = 13,183 t/year; FEN2O = N20 emission factor = 20 g/kg of fertilizer. N20 emission from the use of fertilizer in the Province of Cremona is then:

ECR,N2O = ACR * FEN2O = 13,183 * 20 = 263,660 g/y = 263 kg/y

La surrogated variable used per la disaggregation is the area of ploughed land (hectares):

Total area of ploughed land in the Province of Cremona = 162,896.68 ha Area of ploughed land in the municipality of Dovera = 1,059.02 ha Using (2) N2O emission in the municipality of Dovera is:

EDovera,N2O = ECR,N2O * SupDovera / SupCR = 263 * 1,059 / 162,897 = 1.71 kg/y

Per tornare ai dati rilasciati al pubblico cliccare su:
Dati al pubblico
Per tornare alla pagina inventari delle emissioni cliccare su:
Inventario delle emissioni
per tornare alla gestione dei risultati:
Gestione dei risultati
oppure tornare alla pagina iniziale cliccare su:
Strumento INEMAR

- Commenti (0)

##### Ricerca

##### Quick Links

- Strumento INEMAR
- Progetti INEMAR
- Wiki Fonti

##### Credits

Copyright © ARPA Lombardia
Privacy